==================================================
Trans Computer Maschine Lead Modes Tips and Tricks
==================================================

==============
'Odyssey' mode
==============

The 'Odyssey' mode sets 'Last Note Priority' and enables 'Envelope Retriggering'.

This monophonic mode is featured in many vintage synthesizers including:

ARP Odyssey
KORG MS-20
OSC OSCar (MULT Mode)
Roland SH-101 (Gate+Trig Mode)
Sequential Circuits Pro One (Retrig Mode)


===============
'Minimoog' mode
===============

The 'Minimoog' mode sets 'Low Note Priority' and disables 'Envelope Retriggering'.

This monophonic mode is featured in many vintage synthesizers including:

MOOG Minimoog
MOOG Prodigy
MOOG Source (Single Retrig)
Roland SH-101 (Gate Mode)
Sequential Circuits Pro One (Normal Mode)


===========
'2600' mode
===========

The '2600' mode sets 'Low Note Priority' and enables 'Envelope Retriggering'.

This monophonic mode is featured in many vintage synthesizers including:

ARP 2600
MOOG Source (Multi Retrig)


=============
'Synthi' mode
=============

The 'Synthi' mode sets 'Last Note Priority' and disables 'Envelope Retriggering'.

This monophonic mode is featured in many vintage synthesizers including:

ARP Axxe
EMS Synthi A
EMS Synthi VCS3
OSC OSCar (SG Mode)
Roland SYSTEM-100
Roland TB-303


===============================
Cescato Musiktechnologie © 2018
===============================
